A2. Report Forms L-42 VERSION

CONDUCTED FOR

V = VALID

I = INVALID

N = RESULTS CANNOT BE INTERPRETED (Refer To Comment Section)

Test Number

Stand Run Number:

Oil Code :

Formulation/Stand Code:

Alternate Codes:

In my opinion this test been conducted in a valid manner in accordance with the STP 512A ASTM Test Method and the appropriate amendments through the information letter system. The remarks included in this report describe the anomalies associated with this test.

CMIR or Non-Reference Oil Code

Test Stand:

Date Completed: EOT Time:

SUBMITTED BY: __________________________________________ Testing Laboratory

__________________________________________ Signature

__________________________________________ Typed Name

__________________________________________ Title

__________________________________________ Section

A

A

Fig. A2.1 TEST REPORT COVER

20020220

TEST DATE COMPLETED

END OF TEST TIME TMC OIL NO.

Information Letters Number:

LABORATORY OIL CODE

TOTAL TEST MINUTES

STAND RUN NO. CMIR NO.

Formulation / Stand Code:

SEQ 2 RING

TEST LAB

TEST DATE STARTED

LABORATORY OIL CODE

L-42

FORM 1

TEST RESULT SUMMARY

Discrimination

Calibration Sequence Passing Tests Only

AVERAGE FOR PASSING REFERENCE OIL TESTS

EOT RING

OIL CODE NO.

TEST DATE STARTED

TEST DATE COMPLETED

END OF TEST TIME

TOTAL TEST MINUTES

TEST STAND NO.

STAND RUN NO.

STAND REFERENCE OIL TEST HISTORY IN CHRONOLOGICAL ORDER

Fig. A2.2 TEST RESULT SUMMARY

SEQ 2 RING EOT RING EOT PINION

SEQUENCE 4 SEQUENCE 2

COAST SIDE % SCORING

A

A

COAST SIDE TORQUE (lbf-ft)

EOT PINION

SEQUENCE 4 SEQUENCE 2

COAST SIDE % SCORING COAST SIDE TORQUE (lbf-ft)

Only for non-reference tests. B For non-reference and discrimination tests only.

B

L-42 FORM 2

OPERATIONAL SUMMARY

LAB STAND NO. OIL CODE STAND RUN NO.

GENERAL OPERATION CONDITIONS

1. GEAR LOADING DATA

2. LUBRICANT TEMPERATURE DATA

3. TEST AXLE DATA

SEQUENCE 2 SEQUENCE 4

Drive Side

Coast Side

Torques lbf-ft

Cycle Time Second

Torques lbf-ft

Cycle Time Second Maximum Minimum

Phase

Average Maximum Minimum Average

Specification

Average Value

Minimum Value

Maximum Value Sequence 1* 225 � 5 œF Starting

a. Backlash Initial (in.) Final (in.) Increase (in.)

Maximum Minimum Average

b. Initial Pinion Torque (lbf -in)

Break Turn

RATING DATE RATER INITIALS

Fig. A2.3 OPERATIONAL SUMMARY

Value Sequence 2 Sequence 4

200 � 5 œF < 280 œF

Specification

Maximum Value

* Values after reaching 225 œF

L-42 FORM 3 MEASUREMENT SUMMARY

AXLE CODES

TEST CONDITIONS

INSPECTIONS

ASSEMBLY DATE MATCH NO.

PINION BATCH

RING BATCH

BREAK-IN PROCEDURES DESIGNATION

Acceleration Rate Deceleration Rate

Sequence 2 Unit of Measure Sequence 4 Unit of Measure

Break-In 1st Noise Check 2nd Noise Check Sequence 3 E.O.T.

RING % SCORE PINION % SCORE Drive Side Coast Side Drive Side Coast Side

LAB STAND NO. OIL CODE STAND RUN NO.

Fig. A 2.4 MEASUREMENT SUMMARY

MEASUREMENTS

INITIAL BACKLASH (in.) FINAL BACKLASH (in.)

OPERATOR INIT

OPERATOR INIT

DRIVE SIDE CONTACT PATTERN (Length Rating)

DRIVE SIDE CONTACT PATTERN (Flank Rating)

COAST SIDE CONTACT PATTERN (Length Rating) As Received As Received

As Tested As Tested

As Received As Received

As Tested As Tested

COAST SIDE CONTACT PATTERN (Flank Rating)

L-42 FORM 4 DOWN TIME AND COMMENTS

Number of Downtime Occurrences Test Hours

Date Downtime Reasons

Total Downtime

Other Comments Number of Comment Lines

LAB STAND NO. OIL CODE STAND RUN NO.

Fig. A2.5 DOWN TIME AND COMMENTS