Motion 1:

Move to accept the calibration procedure as provided to replace section 8.3.2.4 with ASTM editorial changes to be implemented prior to the Information Letter.

Motion 2:

Agree to start referencing tests per the proposed matrix using batch A filters per the following Proposal:

* + Run two tests at each laboratory: one test with reference oil  833 and one test with reference oil 832
  + Level 2 alarm system in place
    - Lab runs a third test if **second** test result triggers level 2 alarm
  + Correction factor implemented if all three labs have level 2 alarms in the same direction
  + Allocation:

