From:	Fetterman, Pat [Glen.Fetterman@Infineum.com]
Sent:	Wednesday, September 03, 2008 3:17 PM
To:	a.budd@isp-institute.com; Bill Buscher (E-mail); Bill Larch; Campbell, Bob; Cathy Devlin; charlie.passut@aftonchemical.com; Dan Pridemore; Dick Patrick (E-mail); Glen Fetterman; Greg Miiller; greg.shank@volvo.com; Hind Abi-Akar; James Gutzwiller; James Matasic (E-mail); Jeff Clark; Jesse Hamilton; Jim McGeehan; jim.moritz@intertek.com; Jim Rutherford; joe.franklin@intertek.com; John Haegelin; Keith Selby; kenneth.goshorn@volvo.com; Mark Cooper; Matt Urbanak (E-mail); Norbert Nann (E-mail); Riccardo Conti; Ron Buck; scott cobbs; Scott Harold; Scott Richards (E-mail); Steve Kennedy; Victor Kersey; Wim Van Dam
Subject:	Unconfirmed minutes of our August 28, 2008 teleconference.
Meeting participants:
Ron Buck; Bob Campbell; Jeff Clark; Mark Cooper; Pat Fetterman; Jim Gutzwiller; Ryan Johnson; Jim Moritz; Scott Richards; Jim Rutherford; Greg Shank.

Minutes -
Mark Cooper called the meeting to order at 10:35 am and Greg Shank called in a few minutes later. There was no representative of XOM on the call.
Jim Matasic reported that LZ has a candidate run that has just started and they will then run a reference. Target is mid-September for reference, but could slip.
Jim Moritz reported that Intertek would not run an early reference if it resulted in their losing ability to run on their esisting reference. After clarification, Jim indicated that Intertek will start preparing to run a reference with a target start of the second week in September.
Greg Shank reported that XOM plan to start a reference in early September.
He asle reported that Ken Goshorn has received data that the "new" rings meet all dimensional specs, but he does not have detailed data.
There was an extensive discussion regarding how to use "split" ring sets for candidate oil testing with questions requesting more details regarding how the rings will be placed in test engines to minimize the known cylinder to cylinder wear distribution. Bob Campbell suggested that splitting "new" and "old" rings in cylinders 1,4,5 and 2,3,6 minimized the known offsets, and Scott Richards reported that we had previously run "split" tests during T-12 development using a similar part distribution. Finally, Mark Cooper agreed to prepare an e-mail ballot regarding more details of how to place the ring sets and how to "force" candidate tests to run using "split" hardware. Mark will target to send a proposal during the week of Sept 2.
The next teleconference is planned for Friday, September 12, 2008 at 10:30 am EDT, and a face to face meeting is tentatively planned for the second or third week in October pending the availability of any new reference test data.
Respectfully submitted,
Pat